1、功能说明
    1、TIM3 CH2引脚 CH2上升沿,CH1下降沿计算频率
2、使用环境
    软件开发环境：  KEIL MDK-ARM V5.30.0.0
    硬件环境：      基于N32G030C8L7-STB V1.0开发
3、使用说明
    系统配置：
        1、时钟源：
                    HSE=8M,PLL=48M,AHB=48M,APB1=48M,APB2=48M,TIM3 CLK=48M
        2、中断：
                    TIM3 CH2上升沿 CH1下降沿中断打开，优先级1
        3、端口配置：
                    PA7选择为TIM3 CH2输入
                    PA3选择为IO 输出
        4、TIM：
                    TIM3 CH2上升沿，CH1下降沿捕获中断打开
    使用方法：
        1、编译后打开调试模式，连接PA3与PA7，将变量TIM3Freq、gOnePulsEn添加到watch窗口
        2、默认gOnePulsEn=0，每次手动给gOnePulsEn=1，此时可以看到TIM3Freq计算出来的频率值
4、注意事项
    无

1. Function description
    1. TIM3 CH2 pin, CH2 rising edge, CH1 falling edge to calculate the frequency
2. Use environment
    Software development environment: KEIL MDK-ARM V5.34.0.0
    Hardware environment: Developed based on the evaluation board N32G031C8L7-STB V1.0
3. Instructions for Use
    System configuration：
        1. Clock source:
            HSE=8M, PLL=48M, AHB=48M, APB1=48M, APB2=48M, TIM3 CLK=48M
        2. Interruption:
            TIM3 CH2 rising edge CH1 falling edge interrupt on, priority 1
        3. Port configuration:
            PA7 is selected TIM3 CH2 Input
            PA3 is selected IO Output
        4. TIM:
            TIM3 CH2 rising edge, CH1 falling edge capture interrupt is turned on
Usage method:
    1. Open debugging mode after compilation, connect PA3 to PA7, add variables TIM3Freq, gOnePulsEn to the watch window
    2. Default gOnePulsEn=0, each time you manually give gOnePulsEn=1, you can see the frequency value calculated by TIM3Freq
4. Matters needing attention
    None