1、功能说明

    此例程提供了一种DMA用法，用于在外设与RAM之间传输数据。

2、使用环境

    软件开发环境：
        IDE工具：KEIL MDK-ARM 5.26
    
    硬件环境：
        开发板 N32G43XRL-STB V1.0


3、使用说明
	
    1、时钟源：HSE+PLL
    2、主时钟：108MHz
    3、DMA通道：DMA_CH5，DMA_CH6
    4、I2C1 配置：
            SCL   -->  PB8
            SDA   -->  PB9
            ADDR：0x30(7bit)
            CLOCK：100K
    
    5、I2C2 配置：
            SCL   -->  PB10
            SDA   -->  PB11
            ADDR：0xA0(7bit)
            CLOCK：100K
    
    6、USART1配置：
            TX  -->  PA9
            波特率：115200
            数据位：8bit
            停止位：1bit
            无校验
            
    7、测试步骤与现象
        a，编译下载代码复位运行
        b，从串口看打印信息，验证结果

4、注意事项
    无


1. Function description
    This routine provides a DMA usage for transferring data between peripherals and RAM.

2. Use environment
    Software Development environment:
	IDE tool: KEIL MDK-ARM 5.26   
    Hardware environment:
	Development board N32G43XRL-STB V1.0

3. Instructions for use
    1. Clock source: HSE+PLL
    2. Master clock: 108MHz
    3. DMA channels: DMA_CH5, DMA_CH6
    4. I2C1 configuration:
            	SCL   -->  PB8
            	SDA   -->  PB9
           	ADDR：0x30(7bit)
           	CLOCK：100K   
    5. I2C2 configuration:
            	SCL   -->  PB10
            	SDA   -->  PB11
            	ADDR：0xA0(7bit)
            	CLOCK：100K    
    6. USART1 configuration:
	TX --> PA9
	Baud rate: 115200
	Data bit: 8 bits
	Stop bit: 1bit
	No check            
    7. Test steps and phenomena
	a. Compile download code reset run
	b. View the printed information from the serial port and verify the result

4. Matters needing attention
    None