# Static Call Graph for image .\Objects\CAN_Transmit_Project.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Nov 29 11:37:56 2023

### Maximum Stack Usage = 116 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ USART1_Init ⇒ USART_Init ⇒ RCC_GetClocksFreqValue

### Mutually Recursive functions

- PendSV_Handler ⇒ PendSV_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - BusFault_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - CAN_RX0_IRQHandler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - CAN_RX1_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - CAN_SCE_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - CAN_TX_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - COMP_1_2_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel1_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel2_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel3_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel4_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel5_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel6_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel7_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DMA_Channel8_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - DebugMon_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI0_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI15_10_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI1_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI2_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI3_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI4_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - EXTI9_5_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - FLASH_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - HardFault_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - I2C1_ER_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - I2C1_EV_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - I2C2_ER_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - I2C2_EV_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - LPTIM_WKUP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - LPUART_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - LPUART_WKUP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - MMU_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - MemManage_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - NMI_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - PVD_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - PendSV_Handler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - RAMC_PERR_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - RCC_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - RTCAlarm_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - RTC_WKUP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - Reset_Handler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - SAC_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - SPI1_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - SPI2_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - SVC_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - SysTick_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - SystemInit from system_n32g43x.o(.text) referenced from startup_n32g43x.o(.text)
  - TAMPER_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM1_BRK_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM1_CC_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM1_UP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM2_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM3_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM4_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM5_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM6_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM7_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM8_BRK_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM8_CC_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM8_UP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TIM9_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - TSC_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - UART4_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - UART5_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - UCDR_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - USART1_IRQHandler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - USART2_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - USART3_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - USBWakeUp_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - USB_HP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - USB_LP_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - UsageFault_Handler from n32g43x_it.o(.text) referenced from startup_n32g43x.o(RESET)
  - WWDG_IRQHandler from startup_n32g43x.o(.text) referenced from startup_n32g43x.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_n32g43x.o(.text)
  - fputc from user_usart_config.o(.text) referenced from printf5.o(i.__0printf$5)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_n32g43x.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_n32g43x.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_n32g43x.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  CAN_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  COMP_1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  LPTIM_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  LPUART_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  LPUART_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  MMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  RAMC_PERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  SAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  UCDR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  USB_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  USB_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g43x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  SystemInit (Thumb, 160 bytes, Stack size 8 bytes, system_n32g43x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_n32g43x.o(.text)

  SystemCoreClockUpdate (Thumb, 236 bytes, Stack size 16 bytes, system_n32g43x.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> CAN_NVIC_Config
  - >> NVIC_Configuration

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  CAN_DeInit (Thumb, 24 bytes, Stack size 8 bytes, n32g43x_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_DeInit
  [Calls]
  - >> RCC_EnableAPB1PeriphReset
  [Called By]
  - >> CAN_Config

  CAN_Init (Thumb, 276 bytes, Stack size 12 bytes, n32g43x_can.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CAN_Init
  [Called By]
  - >> CAN_Config

  CAN_InitFilter (Thumb, 258 bytes, Stack size 8 bytes, n32g43x_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_InitFilter
  [Called By]
  - >> CAN_Filter_Init

  CAN_InitStruct (Thumb, 32 bytes, Stack size 0 bytes, n32g43x_can.o(.text))
  [Called By]

  - >> CAN_Config

  CAN_DebugFreeze (Thumb, 22 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_EnTTComMode (Thumb, 118 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_TransmitMessage (Thumb, 294 bytes, Stack size 8 bytes, n32g43x_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_TransmitMessage
  [Called By]
  - >> CANTxMessage

  CAN_TransmitSTS (Thumb, 138 bytes, Stack size 8 bytes, n32g43x_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_TransmitSTS
  [Called By]
  - >> CAN_Tx_Process

  CAN_CancelTransmitMessage (Thumb, 40 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_ReceiveMessage (Thumb, 268 bytes, Stack size 8 bytes, n32g43x_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_ReceiveMessage
  [Called By]
  - >> CAN_RX0_IRQHandler

  CAN_ReleaseFIFO (Thumb, 22 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_PendingMessage (Thumb, 30 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_OperatingModeReq (Thumb, 162 bytes, Stack size 8 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_EnterSleep (Thumb, 30 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_WakeUp (Thumb, 48 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_GetLastErrCode (Thumb, 12 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_GetReceiveErrCounter (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_GetLSBTransmitErrCounter (Thumb, 12 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_INTConfig (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_can.o(.text))
  [Called By]

  - >> CAN_Filter_Init

  CAN_GetFlagSTS (Thumb, 120 bytes, Stack size 8 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_ClearFlag (Thumb, 52 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  CAN_GetIntStatus (Thumb, 284 bytes, Stack size 16 bytes, n32g43x_can.o(.text), UNUSED)
  [Calls]

  - >> CheckINTStatus

  CAN_ClearINTPendingBit (Thumb, 162 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 342 bytes, Stack size 24 bytes, n32g43x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_EnableAPB2PeriphReset

  GPIO_AFIOInitDefault (Thumb, 20 bytes, Stack size 8 bytes, n32g43x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_EnableAPB2PeriphReset

  GPIO_InitPeripheral (Thumb, 484 bytes, Stack size 20 bytes, n32g43x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_InitPeripheral
  [Called By]
  - >> USART1_Init
  - >> LEDInit
  - >> CAN_GPIO_Config

  GPIO_InitStruct (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text))
  [Called By]

  - >> USART1_Init
  - >> LEDInit
  - >> CAN_GPIO_Config

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_SetBitsHigh16 (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ConfigPinLock (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ConfigPinRemap (Thumb, 120 bytes, Stack size 20 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ConfigEventOutput (Thumb, 84 bytes, Stack size 16 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_CtrlEventOutput (Thumb, 6 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  GPIO_ConfigEXTILine (Thumb, 58 bytes, Stack size 12 bytes, n32g43x_gpio.o(.text), UNUSED)

  AFIO_ConfigSPINSSMode (Thumb, 30 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  AFIO_ConfigADCExternalTrigRemap (Thumb, 82 bytes, Stack size 0 bytes, n32g43x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 80 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigHse (Thumb, 70 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitMsiStable
  - >> RCC_WaitHsiStable
  - >> RCC_WaitHseStable

  RCC_WaitHseStable (Thumb, 56 bytes, Stack size 16 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_ConfigHsi (Thumb, 34 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_WaitHsiStable (Thumb, 56 bytes, Stack size 16 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_SetHsiCalibValue (Thumb, 20 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableHsi (Thumb, 6 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigMsi (Thumb, 58 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_WaitMsiStable (Thumb, 56 bytes, Stack size 16 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_SetMsiCalibValue (Thumb, 20 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableMsi (Thumb, 6 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigPll (Thumb, 56 bytes, Stack size 12 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnablePll (Thumb, 6 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigSysclk (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetSysclkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigHclk (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigPclk1 (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigPclk2 (Thumb, 20 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigInt (Thumb, 30 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigUsbClk (Thumb, 16 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigTim18Clk (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigRngcClk (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigAdc1mClk (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigAdcPllClk (Thumb, 30 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigAdcHclk (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigTrng1mClk (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableTrng1mClk (Thumb, 30 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigUCDRClk (Thumb, 46 bytes, Stack size 8 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigUSBXTALESSMode (Thumb, 22 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableRETPeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableRETPeriphReset (Thumb, 62 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableAPB1PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text))
  [Called By]

  - >> CAN_Config
  - >> RCC_ConfigLse
  - >> RCC_ConfigLPTIMClk

  RCC_ConfigLPTIMClk (Thumb, 46 bytes, Stack size 8 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_EnableAPB1PeriphClk

  RCC_GetLPTIMClkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigLPUARTClk (Thumb, 22 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetLPUARTClkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigSRAMParityErrorInt (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigSRAMParityErrorRESET (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ClrSRAMParityErrorFlag (Thumb, 12 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  LSE_XtalConfig (Thumb, 34 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_ConfigLse

  RCC_ConfigLse (Thumb, 102 bytes, Stack size 20 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Calls]

  - >> LSE_XtalConfig
  - >> RCC_EnableAPB1PeriphClk

  RCC_EnableLsi (Thumb, 6 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigRtcClk (Thumb, 22 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetRTCClkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableRtcClk (Thumb, 8 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigLSXClk (Thumb, 22 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetLSXClkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreqValue (Thumb, 302 bytes, Stack size 20 bytes, n32g43x_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreqValue
  [Called By]
  - >> USART_Init

  RCC_EnableAHBPeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableAPB2PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text))
  [Called By]

  - >> USART1_Init
  - >> LEDInit
  - >> CAN_GPIO_Config

  RCC_EnableAHBPeriphReset (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableAPB2PeriphReset (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit
  - >> GPIO_AFIOInitDefault
  - >> GPIO_DeInit

  RCC_EnableAPB1PeriphReset (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text))
  [Called By]

  - >> USART_DeInit
  - >> CAN_DeInit

  RCC_EnableLowPowerReset (Thumb, 8 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableClockSecuritySystem (Thumb, 6 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_EnableLSEClockSecuritySystem (Thumb, 8 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetLSEClockSecuritySystemStatus (Thumb, 20 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigMcoClkPre (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ConfigMco (Thumb, 20 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ClrFlag (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_GetIntStatus (Thumb, 20 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  RCC_ClrIntPendingBit (Thumb, 12 bytes, Stack size 0 bytes, n32g43x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, n32g43x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_EnableAPB2PeriphReset
  - >> RCC_EnableAPB1PeriphReset

  USART_Init (Thumb, 168 bytes, Stack size 56 bytes, n32g43x_usart.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> RCC_GetClocksFreqValue
  [Called By]
  - >> USART1_Init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_Enable (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text))
  [Called By]

  - >> USART1_Init

  USART_ConfigInt (Thumb, 74 bytes, Stack size 20 bytes, n32g43x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ConfigInt
  [Called By]
  - >> USART1_Init

  USART_EnableDMA (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_SetAddr (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_ConfigWakeUpMode (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_EnableRcvWakeUp (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_ConfigLINBreakDetectLength (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_EnableLIN (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, n32g43x_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_EnableSmartCard (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_SetSmartCardNACK (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_EnableHalfDuplex (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_ConfigIrDAMode (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_EnableIrDA (Thumb, 24 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, n32g43x_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ClrFlag (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_usart.o(.text), UNUSED)

  USART_GetIntStatus (Thumb, 84 bytes, Stack size 16 bytes, n32g43x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetIntStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClrIntPendingBit (Thumb, 30 bytes, Stack size 8 bytes, n32g43x_usart.o(.text), UNUSED)

  main (Thumb, 82 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = main ⇒ USART1_Init ⇒ USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> USART1_Init
  - >> Tx_Frame_Message_Init
  - >> Systick_MS_Config
  - >> NVIC_Configuration
  - >> LEDOn
  - >> LEDInit
  - >> CAN_Tx_Process
  - >> CAN_Recieve_Process
  - >> CAN_GPIO_Config
  - >> CAN_Config
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  CAN_GPIO_Config (Thumb, 68 bytes, Stack size 24 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = CAN_GPIO_Config ⇒ GPIO_InitPeripheral
  [Calls]
  - >> RCC_EnableAPB2PeriphClk
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  [Called By]
  - >> main

  CAN_Filter_Init (Thumb, 70 bytes, Stack size 24 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CAN_Filter_Init ⇒ CAN_InitFilter
  [Calls]
  - >> CAN_INTConfig
  - >> CAN_InitFilter
  [Called By]
  - >> CAN_Config

  CAN_NVIC_Config (Thumb, 32 bytes, Stack size 8 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CAN_NVIC_Config ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  [Called By]
  - >> CAN_Config

  CAN_Config (Thumb, 96 bytes, Stack size 16 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = CAN_Config ⇒ CAN_Filter_Init ⇒ CAN_InitFilter
  [Calls]
  - >> CAN_NVIC_Config
  - >> CAN_Filter_Init
  - >> RCC_EnableAPB1PeriphClk
  - >> CAN_InitStruct
  - >> CAN_Init
  - >> CAN_DeInit
  [Called By]
  - >> main

  CANTxMessage (Thumb, 16 bytes, Stack size 16 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CANTxMessage ⇒ CAN_TransmitMessage
  [Calls]
  - >> CAN_TransmitMessage
  [Called By]
  - >> CAN_Tx_Process

  Tx_Frame_Message_Init (Thumb, 102 bytes, Stack size 20 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Tx_Frame_Message_Init
  [Called By]
  - >> main

  CAN_Recieve_Process (Thumb, 174 bytes, Stack size 8 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CAN_Recieve_Process ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> main

  CAN_Tx_Process (Thumb, 98 bytes, Stack size 16 bytes, user_can_config.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = CAN_Tx_Process ⇒ CANTxMessage ⇒ CAN_TransmitMessage
  [Calls]
  - >> User_Time_Set
  - >> User_Time_Read
  - >> CANTxMessage
  - >> CAN_TransmitSTS
  [Called By]
  - >> main

  LEDBlink (Thumb, 8 bytes, Stack size 0 bytes, user_led_config.o(.text), UNUSED)

  LEDOn (Thumb, 4 bytes, Stack size 0 bytes, user_led_config.o(.text))
  [Called By]

  - >> main

  LEDOff (Thumb, 4 bytes, Stack size 0 bytes, user_led_config.o(.text), UNUSED)

  LEDInit (Thumb, 92 bytes, Stack size 32 bytes, user_led_config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = LEDInit ⇒ GPIO_InitPeripheral
  [Calls]
  - >> RCC_EnableAPB2PeriphClk
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  [Called By]
  - >> main

  Systick_MS_Config (Thumb, 88 bytes, Stack size 16 bytes, user_systick_config.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Systick_MS_Config
  [Called By]
  - >> main

  Systick_Disable (Thumb, 18 bytes, Stack size 0 bytes, user_systick_config.o(.text), UNUSED)

  User_Time_Read (Thumb, 30 bytes, Stack size 0 bytes, user_systick_config.o(.text))
  [Called By]

  - >> CAN_Tx_Process

  User_Time_Set (Thumb, 8 bytes, Stack size 0 bytes, user_systick_config.o(.text))
  [Called By]

  - >> CAN_Tx_Process

  NVIC_Configuration (Thumb, 40 bytes, Stack size 8 bytes, user_usart_config.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = NVIC_Configuration ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  USART1_Init (Thumb, 158 bytes, Stack size 40 bytes, user_usart_config.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = USART1_Init ⇒ USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> USART_ConfigInt
  - >> USART_Enable
  - >> USART_Init
  - >> RCC_EnableAPB2PeriphClk
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  [Called By]
  - >> main

  fputc (Thumb, 32 bytes, Stack size 16 bytes, user_usart_config.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Address Reference Count : 1]
  - printf5.o(i.__0printf$5)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  SysTick_Handler (Thumb, 12 bytes, Stack size 0 bytes, n32g43x_it.o(.text))
  [Address Reference Count : 1]

  - startup_n32g43x.o(RESET)

  DMA_IRQ_HANDLER (Thumb, 2 bytes, Stack size 0 bytes, n32g43x_it.o(.text), UNUSED)

  USART1_IRQHandler (Thumb, 54 bytes, Stack size 8 bytes, n32g43x_it.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetIntStatus
  [Calls]
  - >> USART_GetIntStatus
  - >> USART_ReceiveData
  [Address Reference Count : 1]
  - startup_n32g43x.o(RESET)

  CAN_RX0_IRQHandler (Thumb, 48 bytes, Stack size 8 bytes, n32g43x_it.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CAN_RX0_IRQHandler ⇒ CAN_ReceiveMessage
  [Calls]
  - >> CAN_ReceiveMessage
  [Address Reference Count : 1]
  - startup_n32g43x.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __0printf$5 (Thumb, 22 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$5 (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> CAN_Recieve_Process
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 258 bytes, Stack size 12 bytes, system_n32g43x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  CheckINTStatus (Thumb, 18 bytes, Stack size 0 bytes, n32g43x_can.o(.text), UNUSED)
  [Called By]

  - >> CAN_GetIntStatus

  _printf_core (Thumb, 658 bytes, Stack size 104 bytes, printf5.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$5

  ### Undefined Global Symbols