1、功能说明

    此例程展示了通过I2C模块与外部EEPRON的通信。   

2、使用环境

	软件开发环境：
        IDE工具：KEIL MDK-ARM 5.26
    
    硬件环境：
        开发板 N32G43XRL-STB V1.0


3、使用说明
	
    1、时钟源：HSE+PLL
    2、主时钟：108MHz
    3、I2C1 配置：
            SCL   -->  PB6
            SDA   -->  PB7
            ADDR：0xA0(7bit)
            CLOCK:400KHz
            
    4、USART1配置：
            TX  -->  PA9
            波特率：115200
            数据位：8bit
            停止位：1bit
            无校验

    5、测试步骤与现象
        a，检查与外挂EEPROM的连接
        b，编译下载代码复位运行
        c，从串口看打印信息，验证结果

4、注意事项
    a，确保SCL,SDA有外部上拉
    
1. Function description

    This example demonstrates the communication with the external EEPROM through the I2C module.

2. Use environment

    Software development environment:
        IDE tool: KEIL MDK-ARM 5.26
    
    Hardware environment:
        Development board N32G43XRL-STB V1.0


3. Instructions for use

    1. Clock source: HSE+PLL
    2. Main clock: 108MHz
    3. I2C1 configuration:
            SCL --> PB6 
            SDA --> PB7 

            ADDR: 0xA0(7bit)
            CLOCK: 400KHz
            
    4. USART1 configuration:
            TX --> PA9 50MHz, AF_PP
            Baud rate: 115200
            Data bit: 8bit
            Stop bit: 1bit
            No verification

    5. Test steps and phenomena
        a, check the EEPROM connection
        b, compile and download the code, reset and run
        c, view the print information from the serial port and verify the result

4. Matters needing attention
    1. Ensure that SCL\SDA has an external pull-up