1、功能说明

    /* 简单描述工程功能 */
        这个例程配置并演示bitband位带操作


2、使用环境

        软件开发环境：KEIL MDK-ARM V5.34.0.0
                      IAR EWARM 8.50.1
    
        硬件环境：基于评估板N32G430C8L7-STB V1.0开发


3、使用说明

    /* 描述相关模块配置方法；例如:时钟，I/O等 */
        SystemClock：128MHz
        USART：TX - PA9，RX - PA10，波特率115200

    /* 描述Demo的测试步骤和现象 */
        1.编译后下载程序复位运行；
        2.对32位数据的不同位进行置1置0操作，再读取写入值与读取值，查看打印信息；


4、注意事项


1. Function description
    /* A brief description of the engineering function */
    This routine configures and demonstrates the bitBand bitband operation
2. Use environment

    Software development environment: KEIL MDK-ARM V5.34.0.0
                                          IAR EWARM 8.50.1
    Hardware environment: Developed based on the evaluation board N32G430C8L7-STB V1.0

3. Instructions for use
    
    /* Describe the related module configuration method; For example: clock, I/O, etc. */
    SystemClock: 128MHZ
    USART: TX-PA9, RX-PA10, baud rate 115200
    /* Describes the test steps and symptoms of Demo */
    1. Reset and run the downloaded program after compilation;
    2. Set 1 to 0 for different bits of 32-bit data, read the write value and read value, and view the printed information.
4. Precautions
    None