1、功能说明
    1、通过EXTI线来触发日历打印输出。

2、使用环境

    软件开发环境：KEIL MDK-ARM V5.34.0.0
                  IAR EWARM 8.50.1
    硬件环境：基于评估板N32G430C8L7-STB V1.0开发

3、使用说明
    
    系统配置:
        1、RTC时钟源：LSE 32.768kHz
        2、中断线：EXTI_LINE7--PA7
        3、串口配置：
                    - 串口为USART1（TX：PA9）:
                    - 数据位：8
                    - 停止位：1
                    - 奇偶校验：无
                    - 波特率： 115200 
    使用方法：
        编译后烧录到评估板，PC13连接到PA7口，上电后，串口每隔1S会打印一次对应日历时间

4、注意事项
    无


1. Function description
    1. Trigger the calendar print through the EXTI line.

2. Use environment
    Software development environment: KEIL MDK-ARM V5.34.0.0
                                      IAR EWARM 8.50.1
    Hardware environment: Developed based on the evaluation board N32G430C8L7-STB V1.0​

3. Instructions for use

    System Configuration;
        1. RTC clock source: LSE 32.768kHz
        2. Interrupt line: EXTI_LINE7--PA7
        3. Serial port configuration:
                            - Serial port is USART1 (TX: PA9)
                            - Data bits: 8
                            - Stop bit: 1
                            - Parity: none
                            - Baud rate: 115200

    Instructions:
        After compiling and burning it to the evaluation board, PC13 is connected to the PA7 port. After power-on, the serial port will print the corresponding calendar time every 1 second.


4. Attention
    none