1、功能说明
    1、ADC采样、转换PA0引脚的模拟电压
    2、其中ADC转换结果通过DMA_CH1通道读取到变量ADCConvertedValue
2、使用环境
    
       软件开发环境：  
          IDE工具：KEIL MDK-ARM V5.34.0.0
                         IAR EWARM 8.50.1

       硬件环境：      
          开发板：N32G430C8L7-STB V1.0

3、使用说明
    系统配置；
        1、时钟源：
            HSE=8M,PLL=128M,AHB=128M,APB1=32M,APB2=64M,ADC CLK=128M/16,ADC 1M CLK=HSE/8
        2、端口配置：
            PA0选择为模拟功能ADC转换通道1
        3、DMA：
            DMA_CH1通道循环模式搬运一个半字的ADC转换结果到ADCConvertedValue变量
        4、ADC：
            ADC连续转换、扫描模式、软件触发、12位数据右对齐，转换通道1即PA0的模拟电压数据
    使用方法：
        1、编译后打开调试模式，将变量ADCConvertedValue添加到watch窗口观察
        2、通过改变PA0引脚的电压，可以看到转换结果变量同步改变
4、注意事项
    当系统采用HSE时钟时（一般HSI也是打开的），RCC_ConfigAdc1mClk(RCC_ADC1MCLK_SRC_HSE, RCC_ADC1MCLK_DIV8)可以配置为HSE或者HSI
    当系统采样HSI时钟时（一般HSE是关闭的），RCC_ConfigAdc1mClk(RCC_ADC1MCLK_SRC_HSI, RCC_ADC1MCLK_DIV8)只能配置为HSI



1. Function description
    1. ADC samples and converts the analog voltage of PA0 pin
    2. ADC conversion results are read to variable ADCConvertedValue through DMA_CH1 channel
2. Use environment
    Software development environment:   KEIL MDK-ARM V5.34.0.0
                                                                IAR EWARM 8.50.1
    Hardware environment: 
        the evaluation board:   N32G430C8L7-STB V1.0

3. Instructions for use
    System configuration：
       1. Clock source:
              HSE=8M,PLL=128M,AHB=128M,APB1=32M,APB2=64M,ADC CLK=128M/16,ADC 1M CLK=HSE/8
       2. Port Configuration:
              PA0 is selected as the analog function ADC conversion channel 1
       3. the DMA:
              DMA_CH1 channel loopback mode carries a half-word ADC conversion result to the ADCConvertedValue variable
       4. the ADC:
              ADC continuous conversion, scan mode, software trigger, 12 bit data right aligned, conversion channel 1 is PA0 analog voltage data
    Usage:
       1. After compiling, open the debugging mode and add the variable ADCConvertedValue to the Watch window 
           for observation.
       2. By changing the voltage of the PA0 pin, you can see that the conversion result variable changes synchronously
4. Precautions
       When the system uses the HSE clock (HSI is also normally turned on), RCC_ConfigAdc1mClk(RCC_ADC1MCLK_SRC_HSE, 
       RCC_ADC1MCLK_DIV8)can be configured as HSE or HSI.
       When the system samples the HSI clock (generally, HSE is disabled), RCC_ConfigAdc1mClk(RCC_ADC1MCLK_SRC_HSI, 
       RCC_ADC1MCLK_DIV8) can only be set to HSI.