# Static Call Graph for image .\Objects\LP_RUN.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Mon Apr 15 11:13:09 2024

### Maximum Stack Usage = 116 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ log_init ⇒ USART_Init ⇒ RCC_GetClocksFreqValue

### Mutually Recursive functions

- PendSV_Handler ⇒ PendSV_Handler
- CAN_RX0_IRQHandler ⇒ CAN_RX0_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from n32l40x_it.o(i.ADC_IRQHandler) referenced from startup_n32l40x.o(RESET)
  - BusFault_Handler from n32l40x_it.o(i.BusFault_Handler) referenced from startup_n32l40x.o(RESET)
  - CAN_RX0_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - CAN_RX1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - CAN_SCE_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - CAN_TX_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - COMP_1_2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel6_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel7_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel8_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DebugMon_Handler from n32l40x_it.o(i.DebugMon_Handler) referenced from startup_n32l40x.o(RESET)
  - EXTI0_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI15_10_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI9_5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - FLASH_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - HardFault_Handler from n32l40x_it.o(i.HardFault_Handler) referenced from startup_n32l40x.o(RESET)
  - I2C1_ER_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - I2C1_EV_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - I2C2_ER_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - I2C2_EV_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LCD_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LPTIM_WKUP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LPUART_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LPUART_WKUP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - MMU_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - MemManage_Handler from n32l40x_it.o(i.MemManage_Handler) referenced from startup_n32l40x.o(RESET)
  - NMI_Handler from n32l40x_it.o(i.NMI_Handler) referenced from startup_n32l40x.o(RESET)
  - PVD_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - PendSV_Handler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RAMC_PERR_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RCC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RTCAlarm_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RTC_WKUP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - Reset_Handler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SAC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SPI1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SPI2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SVC_Handler from n32l40x_it.o(i.SVC_Handler) referenced from startup_n32l40x.o(RESET)
  - SysTick_Handler from n32l40x_it.o(i.SysTick_Handler) referenced from startup_n32l40x.o(RESET)
  - SystemInit from system_n32l40x.o(i.SystemInit) referenced from startup_n32l40x.o(.text)
  - TAMPER_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_BRK_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_CC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_UP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM6_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM7_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_BRK_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_CC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_UP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM9_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TSC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UART4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UART5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UCDR_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USART1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USART2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USART3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USBWakeUp_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USB_HP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USB_LP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UsageFault_Handler from n32l40x_it.o(i.UsageFault_Handler) referenced from startup_n32l40x.o(RESET)
  - WWDG_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_n32l40x.o(.text)
  - fputc from log.o(i.fputc) referenced from printf1.o(i.__0printf$1)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_n32l40x.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_n32l40x.o(RESET)

  CAN_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Calls]

  - >> CAN_RX0_IRQHandler
  [Called By]
  - >> CAN_RX0_IRQHandler
  [Address Reference Count : 1]
  - startup_n32l40x.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  CAN_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  COMP_1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LPTIM_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LPUART_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LPUART_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  MMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RAMC_PERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  UCDR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USB_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USB_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  ADC_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_ClearFlag))
  [Called By]

  - >> ADC_GetData

  ADC_ConfigClk (Thumb, 42 bytes, Stack size 16 bytes, n32l40x_adc.o(i.ADC_ConfigClk))
  [Stack]

  - Max Depth = 16
  - Call Chain = ADC_ConfigClk
  [Calls]
  - >> RCC_ConfigAdcPllClk
  - >> RCC_ConfigAdcHclk
  [Called By]
  - >> RCC_Configuration

  ADC_ConfigInt (Thumb, 24 bytes, Stack size 8 bytes, n32l40x_adc.o(i.ADC_ConfigInt))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_ConfigInt
  [Called By]
  - >> ADC_Initial

  ADC_ConfigRegularChannel (Thumb, 198 bytes, Stack size 20 bytes, n32l40x_adc.o(i.ADC_ConfigRegularChannel))
  [Stack]

  - Max Depth = 20
  - Call Chain = ADC_ConfigRegularChannel
  [Called By]
  - >> ADC_GetData

  ADC_DeInit (Thumb, 28 bytes, Stack size 8 bytes, n32l40x_adc.o(i.ADC_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DeInit
  [Calls]
  - >> RCC_EnableAHBPeriphReset
  [Called By]
  - >> ADC_Initial

  ADC_Enable (Thumb, 36 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_Enable))
  [Called By]

  - >> ADC_Initial

  ADC_EnableSoftwareStartConv (Thumb, 22 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_EnableSoftwareStartConv))
  [Called By]

  - >> ADC_GetData

  ADC_GetCalibrationStatus (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_GetCalibrationStatus))
  [Called By]

  - >> ADC_Initial

  ADC_GetDat (Thumb, 8 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_GetDat))
  [Called By]

  - >> ADC_GetData

  ADC_GetData (Thumb, 66 bytes, Stack size 16 bytes, main.o(i.ADC_GetData))
  [Stack]

  - Max Depth = 36
  - Call Chain = ADC_GetData ⇒ ADC_ConfigRegularChannel
  [Calls]
  - >> ADC_GetFlagStatus
  - >> ADC_GetDat
  - >> ADC_EnableSoftwareStartConv
  - >> ADC_ConfigRegularChannel
  - >> ADC_ClearFlag
  [Called By]
  - >> main

  ADC_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_GetFlagStatus))
  [Called By]

  - >> ADC_GetData

  ADC_GetFlagStatusNew (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_GetFlagStatusNew))
  [Called By]

  - >> ADC_Initial

  ADC_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, n32l40x_it.o(i.ADC_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_IRQHandler
  [Calls]
  - >> GPIO_WriteBit
  [Address Reference Count : 1]
  - startup_n32l40x.o(RESET)

  ADC_Init (Thumb, 78 bytes, Stack size 12 bytes, n32l40x_adc.o(i.ADC_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = ADC_Init
  [Called By]
  - >> ADC_Initial

  ADC_Initial (Thumb, 118 bytes, Stack size 8 bytes, main.o(i.ADC_Initial))
  [Stack]

  - Max Depth = 24
  - Call Chain = ADC_Initial ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> ADC_StartCalibration
  - >> ADC_Init
  - >> ADC_GetFlagStatusNew
  - >> ADC_GetCalibrationStatus
  - >> ADC_Enable
  - >> ADC_DeInit
  - >> ADC_ConfigInt
  [Called By]
  - >> main

  ADC_StartCalibration (Thumb, 28 bytes, Stack size 0 bytes, n32l40x_adc.o(i.ADC_StartCalibration))
  [Called By]

  - >> ADC_Initial

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  ConfigMRVoltage1V (Thumb, 124 bytes, Stack size 0 bytes, system_n32l40x.o(i.ConfigMRVoltage1V))
  [Called By]

  - >> SetSysClock

  DBG_ConfigPeriph (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_dbg.o(i.DBG_ConfigPeriph))
  [Called By]

  - >> main

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  Delay_ms (Thumb, 26 bytes, Stack size 0 bytes, main.o(i.Delay_ms))
  [Called By]

  - >> main

  FLASH_PrefetchBufSet (Thumb, 22 bytes, Stack size 0 bytes, n32l40x_flash.o(i.FLASH_PrefetchBufSet))
  [Called By]

  - >> SetSysClock_MSI

  FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_flash.o(i.FLASH_SetLatency))
  [Called By]

  - >> SetSysClockToPLL
  - >> PWR_ExitLowPowerRunMode
  - >> PWR_EnterLowPowerRunMode

  GPIO_Configuration (Thumb, 74 bytes, Stack size 24 bytes, main.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 44
  - Call Chain = GPIO_Configuration ⇒ GPIO_InitPeripheral
  [Calls]
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  [Called By]
  - >> main

  GPIO_InitPeripheral (Thumb, 484 bytes, Stack size 20 bytes, n32l40x_gpio.o(i.GPIO_InitPeripheral))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_InitPeripheral
  [Called By]
  - >> log_init
  - >> LEDInit
  - >> GPIO_Configuration

  GPIO_InitStruct (Thumb, 24 bytes, Stack size 0 bytes, n32l40x_gpio.o(i.GPIO_InitStruct))
  [Called By]

  - >> log_init
  - >> LEDInit
  - >> GPIO_Configuration

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, n32l40x_gpio.o(i.GPIO_WriteBit))
  [Called By]

  - >> ADC_IRQHandler

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LEDBlink (Thumb, 8 bytes, Stack size 0 bytes, user_led_config.o(i.LEDBlink))
  [Called By]

  - >> main

  LEDInit (Thumb, 92 bytes, Stack size 32 bytes, user_led_config.o(i.LEDInit))
  [Stack]

  - Max Depth = 52
  - Call Chain = LEDInit ⇒ GPIO_InitPeripheral
  [Calls]
  - >> RCC_EnableAPB2PeriphClk
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  [Called By]
  - >> main

  LEDOff (Thumb, 4 bytes, Stack size 0 bytes, user_led_config.o(i.LEDOff))
  [Called By]

  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> ADC_Initial

  PWR_EnterLowPowerRunMode (Thumb, 142 bytes, Stack size 8 bytes, n32l40x_pwr.o(i.PWR_EnterLowPowerRunMode))
  [Stack]

  - Max Depth = 40
  - Call Chain = PWR_EnterLowPowerRunMode ⇒ SetSysClock_MSI ⇒ RCC_WaitMsiStable ⇒ RCC_GetFlagStatus
  [Calls]
  - >> FLASH_SetLatency
  - >> SetSysClock_MSI
  [Called By]
  - >> main

  PWR_ExitLowPowerRunMode (Thumb, 236 bytes, Stack size 8 bytes, n32l40x_pwr.o(i.PWR_ExitLowPowerRunMode))
  [Stack]

  - Max Depth = 8
  - Call Chain = PWR_ExitLowPowerRunMode
  [Calls]
  - >> FLASH_SetLatency
  [Called By]
  - >> main

  RCC_ConfigAdc1mClk (Thumb, 24 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigAdc1mClk))
  [Called By]

  - >> RCC_Configuration

  RCC_ConfigAdcHclk (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigAdcHclk))
  [Called By]

  - >> ADC_ConfigClk

  RCC_ConfigAdcPllClk (Thumb, 30 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigAdcPllClk))
  [Called By]

  - >> ADC_ConfigClk

  RCC_ConfigHclk (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigHclk))
  [Called By]

  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_ConfigHse (Thumb, 70 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigHse))
  [Called By]

  - >> SetSysClockToPLL

  RCC_ConfigHsi (Thumb, 34 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigHsi))
  [Called By]

  - >> SetSysClockToPLL

  RCC_ConfigMsi (Thumb, 58 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigMsi))
  [Called By]

  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_ConfigPclk1 (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigPclk1))
  [Called By]

  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_ConfigPclk2 (Thumb, 20 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigPclk2))
  [Called By]

  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_ConfigPll (Thumb, 56 bytes, Stack size 12 bytes, n32l40x_rcc.o(i.RCC_ConfigPll))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_ConfigPll
  [Called By]
  - >> SetSysClockToPLL

  RCC_ConfigSysclk (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_ConfigSysclk))
  [Called By]

  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_Configuration (Thumb, 40 bytes, Stack size 8 bytes, main.o(i.RCC_Configuration))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_Configuration ⇒ ADC_ConfigClk
  [Calls]
  - >> RCC_EnableAPB2PeriphClk
  - >> RCC_EnableAHBPeriphClk
  - >> RCC_ConfigAdc1mClk
  - >> ADC_ConfigClk
  [Called By]
  - >> main

  RCC_DeInit (Thumb, 80 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_DeInit))
  [Called By]

  - >> SetSysClock_MSI

  RCC_EnableAHBPeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnableAHBPeriphClk))
  [Called By]

  - >> RCC_Configuration

  RCC_EnableAHBPeriphReset (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnableAHBPeriphReset))
  [Called By]

  - >> ADC_DeInit

  RCC_EnableAPB1PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnableAPB1PeriphClk))
  [Called By]

  - >> main

  RCC_EnableAPB2PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnableAPB2PeriphClk))
  [Called By]

  - >> log_init
  - >> LEDInit
  - >> RCC_Configuration

  RCC_EnablePll (Thumb, 6 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnablePll))
  [Called By]

  - >> SetSysClockToPLL

  RCC_GetClocksFreqValue (Thumb, 302 bytes, Stack size 20 bytes, n32l40x_rcc.o(i.RCC_GetClocksFreqValue))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreqValue
  [Called By]
  - >> USART_Init

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, n32l40x_rcc.o(i.RCC_GetFlagStatus))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetFlagStatus
  [Called By]
  - >> RCC_WaitMsiStable
  - >> RCC_WaitHsiStable
  - >> RCC_WaitHseStable
  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_GetSysclkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_GetSysclkSrc))
  [Called By]

  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  RCC_WaitHseStable (Thumb, 56 bytes, Stack size 16 bytes, n32l40x_rcc.o(i.RCC_WaitHseStable))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_WaitHseStable ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> SetSysClockToPLL

  RCC_WaitHsiStable (Thumb, 56 bytes, Stack size 16 bytes, n32l40x_rcc.o(i.RCC_WaitHsiStable))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_WaitHsiStable ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> SetSysClockToPLL

  RCC_WaitMsiStable (Thumb, 56 bytes, Stack size 16 bytes, n32l40x_rcc.o(i.RCC_WaitMsiStable))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_WaitMsiStable ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> SetSysClockToPLL
  - >> SetSysClock_MSI

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SetSysClockToPLL (Thumb, 422 bytes, Stack size 56 bytes, user_sysclock_config.o(i.SetSysClockToPLL))
  [Stack]

  - Max Depth = 80
  - Call Chain = SetSysClockToPLL ⇒ RCC_WaitMsiStable ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_WaitMsiStable
  - >> RCC_WaitHsiStable
  - >> RCC_WaitHseStable
  - >> RCC_GetSysclkSrc
  - >> RCC_GetFlagStatus
  - >> RCC_EnablePll
  - >> RCC_ConfigSysclk
  - >> RCC_ConfigPll
  - >> RCC_ConfigPclk2
  - >> RCC_ConfigPclk1
  - >> RCC_ConfigMsi
  - >> RCC_ConfigHsi
  - >> RCC_ConfigHse
  - >> RCC_ConfigHclk
  - >> FLASH_SetLatency
  [Called By]
  - >> main

  SetSysClock_MSI (Thumb, 72 bytes, Stack size 8 bytes, n32l40x_pwr.o(i.SetSysClock_MSI))
  [Stack]

  - Max Depth = 32
  - Call Chain = SetSysClock_MSI ⇒ RCC_WaitMsiStable ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_WaitMsiStable
  - >> RCC_GetSysclkSrc
  - >> RCC_GetFlagStatus
  - >> RCC_ConfigSysclk
  - >> RCC_ConfigPclk2
  - >> RCC_ConfigPclk1
  - >> RCC_ConfigMsi
  - >> RCC_ConfigHclk
  - >> FLASH_PrefetchBufSet
  - >> RCC_DeInit
  [Called By]
  - >> PWR_EnterLowPowerRunMode

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SystemInit (Thumb, 190 bytes, Stack size 8 bytes, system_n32l40x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_n32l40x.o(.text)

  USART_Enable (Thumb, 24 bytes, Stack size 0 bytes, n32l40x_usart.o(i.USART_Enable))
  [Called By]

  - >> log_init

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> fputc

  USART_Init (Thumb, 168 bytes, Stack size 56 bytes, n32l40x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> RCC_GetClocksFreqValue
  [Called By]
  - >> log_init

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, n32l40x_usart.o(i.USART_SendData))
  [Called By]

  - >> fputc

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  __0printf$1 (Thumb, 22 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$1 (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 90 bytes, Stack size 16 bytes, log.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - printf1.o(i.__0printf$1)

  log_init (Thumb, 106 bytes, Stack size 40 bytes, log.o(i.log_init))
  [Stack]

  - Max Depth = 116
  - Call Chain = log_init ⇒ USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> RCC_EnableAPB2PeriphClk
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  - >> USART_Init
  - >> USART_Enable
  [Called By]
  - >> main

  main (Thumb, 330 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 116
  - Call Chain = main ⇒ log_init ⇒ USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> log_init
  - >> SetSysClockToPLL
  - >> RCC_EnableAPB1PeriphClk
  - >> PWR_ExitLowPowerRunMode
  - >> PWR_EnterLowPowerRunMode
  - >> LEDOff
  - >> LEDInit
  - >> LEDBlink
  - >> DBG_ConfigPeriph
  - >> RCC_Configuration
  - >> GPIO_Configuration
  - >> Delay_ms
  - >> ADC_Initial
  - >> ADC_GetData
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetSysClock (Thumb, 222 bytes, Stack size 20 bytes, system_n32l40x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock
  [Calls]
  - >> ConfigMRVoltage1V
  [Called By]
  - >> SystemInit

  _printf_core (Thumb, 336 bytes, Stack size 88 bytes, printf1.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  [Called By]
  - >> __0printf$1

  ### Undefined Global Symbols