# Static Call Graph for image .\Objects\TIM1_Synchro.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Nov 08 14:31:18 2023

### Maximum Stack Usage = 44 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ GPIO_Configuration ⇒ GPIO_InitPeripheral

### Mutually Recursive functions

- PendSV_Handler ⇒ PendSV_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - BusFault_Handler from n32l40x_it.o(i.BusFault_Handler) referenced from startup_n32l40x.o(RESET)
  - CAN_RX0_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - CAN_RX1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - CAN_SCE_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - CAN_TX_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - COMP_1_2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel6_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel7_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DMA_Channel8_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - DebugMon_Handler from n32l40x_it.o(i.DebugMon_Handler) referenced from startup_n32l40x.o(RESET)
  - EXTI0_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI15_10_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - EXTI9_5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - FLASH_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - HardFault_Handler from n32l40x_it.o(i.HardFault_Handler) referenced from startup_n32l40x.o(RESET)
  - I2C1_ER_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - I2C1_EV_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - I2C2_ER_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - I2C2_EV_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LCD_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LPTIM_WKUP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LPUART_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - LPUART_WKUP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - MMU_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - MemManage_Handler from n32l40x_it.o(i.MemManage_Handler) referenced from startup_n32l40x.o(RESET)
  - NMI_Handler from n32l40x_it.o(i.NMI_Handler) referenced from startup_n32l40x.o(RESET)
  - PVD_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - PendSV_Handler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RAMC_PERR_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RCC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RTCAlarm_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - RTC_WKUP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - Reset_Handler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SAC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SPI1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SPI2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - SVC_Handler from n32l40x_it.o(i.SVC_Handler) referenced from startup_n32l40x.o(RESET)
  - SysTick_Handler from n32l40x_it.o(i.SysTick_Handler) referenced from startup_n32l40x.o(RESET)
  - SystemInit from system_n32l40x.o(i.SystemInit) referenced from startup_n32l40x.o(.text)
  - TAMPER_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_BRK_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_CC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM1_UP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM6_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM7_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_BRK_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_CC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM8_UP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TIM9_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - TSC_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UART4_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UART5_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UCDR_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USART1_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USART2_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USART3_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USBWakeUp_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USB_HP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - USB_LP_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - UsageFault_Handler from n32l40x_it.o(i.UsageFault_Handler) referenced from startup_n32l40x.o(RESET)
  - WWDG_IRQHandler from startup_n32l40x.o(.text) referenced from startup_n32l40x.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_n32l40x.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_n32l40x.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_n32l40x.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_n32l40x.o(RESET)

  CAN_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  CAN_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  COMP_1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  DMA_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LPTIM_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LPUART_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  LPUART_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  MMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RAMC_PERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  UCDR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USB_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  USB_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32l40x.o(.text))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  ConfigMRVoltage1V (Thumb, 124 bytes, Stack size 0 bytes, system_n32l40x.o(i.ConfigMRVoltage1V))
  [Called By]

  - >> SetSysClock

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  GPIO_Configuration (Thumb, 76 bytes, Stack size 24 bytes, main.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 44
  - Call Chain = GPIO_Configuration ⇒ GPIO_InitPeripheral
  [Calls]
  - >> GPIO_InitStruct
  - >> GPIO_InitPeripheral
  [Called By]
  - >> main

  GPIO_InitPeripheral (Thumb, 484 bytes, Stack size 20 bytes, n32l40x_gpio.o(i.GPIO_InitPeripheral))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_InitPeripheral
  [Called By]
  - >> GPIO_Configuration

  GPIO_InitStruct (Thumb, 24 bytes, Stack size 0 bytes, n32l40x_gpio.o(i.GPIO_InitStruct))
  [Called By]

  - >> GPIO_Configuration

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  RCC_Configuration (Thumb, 22 bytes, Stack size 8 bytes, main.o(i.RCC_Configuration))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_Configuration
  [Calls]
  - >> RCC_EnableAPB1PeriphClk
  - >> RCC_EnableAPB2PeriphClk
  [Called By]
  - >> main

  RCC_EnableAPB1PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnableAPB1PeriphClk))
  [Called By]

  - >> RCC_Configuration

  RCC_EnableAPB2PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32l40x_rcc.o(i.RCC_EnableAPB2PeriphClk))
  [Called By]

  - >> RCC_Configuration

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32l40x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  SystemInit (Thumb, 190 bytes, Stack size 8 bytes, system_n32l40x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_n32l40x.o(.text)

  TIM_ConfigBkdt (Thumb, 82 bytes, Stack size 8 bytes, n32l40x_tim.o(i.TIM_ConfigBkdt))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ConfigBkdt
  [Called By]
  - >> main

  TIM_Enable (Thumb, 22 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_Enable))
  [Called By]

  - >> main

  TIM_EnableCtrlPwmOutputs (Thumb, 30 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_EnableCtrlPwmOutputs))
  [Called By]

  - >> main

  TIM_InitBkdtStruct (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_InitBkdtStruct))
  [Called By]

  - >> main

  TIM_InitOc1 (Thumb, 106 bytes, Stack size 12 bytes, n32l40x_tim.o(i.TIM_InitOc1))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_InitOc1
  [Called By]
  - >> main

  TIM_InitOcStruct (Thumb, 20 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_InitOcStruct))
  [Called By]

  - >> main

  TIM_InitTimBaseStruct (Thumb, 30 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_InitTimBaseStruct))
  [Called By]

  - >> main

  TIM_InitTimeBase (Thumb, 296 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_InitTimeBase))
  [Called By]

  - >> main

  TIM_SelectInputTrig (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_SelectInputTrig))
  [Called By]

  - >> main

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_SelectMasterSlaveMode))
  [Called By]

  - >> main

  TIM_SelectOutputTrig (Thumb, 16 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_SelectOutputTrig))
  [Called By]

  - >> main

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, n32l40x_tim.o(i.TIM_SelectSlaveMode))
  [Called By]

  - >> main

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32l40x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_n32l40x.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 292 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 44
  - Call Chain = main ⇒ GPIO_Configuration ⇒ GPIO_InitPeripheral
  [Calls]
  - >> RCC_Configuration
  - >> GPIO_Configuration
  - >> TIM_SelectSlaveMode
  - >> TIM_SelectOutputTrig
  - >> TIM_SelectMasterSlaveMode
  - >> TIM_SelectInputTrig
  - >> TIM_InitTimeBase
  - >> TIM_InitTimBaseStruct
  - >> TIM_InitOcStruct
  - >> TIM_InitOc1
  - >> TIM_InitBkdtStruct
  - >> TIM_EnableCtrlPwmOutputs
  - >> TIM_Enable
  - >> TIM_ConfigBkdt
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetSysClock (Thumb, 222 bytes, Stack size 20 bytes, system_n32l40x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock
  [Calls]
  - >> ConfigMRVoltage1V
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols