# Static Call Graph for image .\Objects\LedBlink.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Mon Apr 29 13:44:55 2024

### Maximum Stack Usage = 60 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ LED_Init ⇒ GPIO_InitPeripheral

### Mutually Recursive functions

- PendSV_Handler ⇒ PendSV_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ADC3_ADC4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM1_BRK_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM1_CC_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM1_TRG_COM_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM1_UP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM2_BRK_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM2_CC_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM2_TRG_COM_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM2_UP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM3_BRK_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM3_CC_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM3_TRG_COM_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ATIM3_UP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - BTIM1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - BTIM2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - BusFault_Handler from n32h47x_48x_it.o(i.BusFault_Handler) referenced from startup_n32h487.o(RESET)
  - Cordic_IRQ_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DAC1_2_3_4_Underflow_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DAC5_6_7_8_Underflow_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA1_Channel8_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel6_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel7_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DMA2_Channel8_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DVP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - DebugMon_Handler from n32h47x_48x_it.o(i.DebugMon_Handler) referenced from startup_n32h487.o(RESET)
  - ETH_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - ETH_WKUP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI0_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI15_10_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI3_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - EXTI9_5_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FDCAN1_INT0_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FDCAN1_INT1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FDCAN2_INT0_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FDCAN2_INT1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FDCAN3_INT0_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FDCAN3_INT1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FEMC_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FLASH_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - FMAC_IRQ_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM10_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM3_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM5_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM6_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM7_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM8_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - GTIM9_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - HardFault_Handler from n32h47x_48x_it.o(i.HardFault_Handler) referenced from startup_n32h487.o(RESET)
  - I2C1_ER_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C1_EV_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C2_ER_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C2_EV_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C3_ER_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C3_EV_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C4_ER_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - I2C4_EV_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - LPTIM1_WKUP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - LPTIM2_WKUP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - MemManage_Handler from n32h47x_48x_it.o(i.MemManage_Handler) referenced from startup_n32h487.o(RESET)
  - NMI_Handler from n32h47x_48x_it.o(i.NMI_Handler) referenced from startup_n32h487.o(RESET)
  - PVD_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - PendSV_Handler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - RCC_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - RTCAlarm_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - RTC_TAMPER_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - RTC_WKUP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - Reset_Handler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SAC_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SDIO_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SMPU_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SPI1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SPI2_I2S2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SPI3_I2S3_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SPI4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SPI5_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SPI6_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SRAM_ERR_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - SVC_Handler from n32h47x_48x_it.o(i.SVC_Handler) referenced from startup_n32h487.o(RESET)
  - SysTick_Handler from n32h47x_48x_it.o(i.SysTick_Handler) referenced from startup_n32h487.o(RESET)
  - SystemInit from system_n32h47x_48x.o(i.SystemInit) referenced from startup_n32h487.o(.text)
  - UART5_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - UART6_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - UART7_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - UART8_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - UCDR_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USART1_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USART2_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USART3_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USART4_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_FS_HP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_FS_LP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_FS_WKUP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_HS_EPx_IN_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_HS_EPx_OUT_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_HS_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - USB_HS_WKUP_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - UsageFault_Handler from n32h47x_48x_it.o(i.UsageFault_Handler) referenced from startup_n32h487.o(RESET)
  - WWDG_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - XSPI_IRQHandler from startup_n32h487.o(.text) referenced from startup_n32h487.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_n32h487.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_n32h487.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_n32h487.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_n32h487.o(RESET)

  ADC3_ADC4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM2_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM2_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM2_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM2_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM3_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM3_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM3_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ATIM3_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  BTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  BTIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  Cordic_IRQ_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DAC1_2_3_4_Underflow_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DAC5_6_7_8_Underflow_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA1_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DMA2_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DVP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FDCAN1_INT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FDCAN1_INT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FDCAN2_INT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FDCAN2_INT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FDCAN3_INT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FDCAN3_INT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FEMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  FMAC_IRQ_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  GTIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C4_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  I2C4_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  LPTIM1_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  LPTIM2_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  RTC_TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SMPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SPI2_I2S2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SPI3_I2S3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SRAM_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  UART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  UCDR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_FS_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_FS_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_HS_EPx_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_HS_EPx_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  USB_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  XSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32h487.o(.text))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  Delay (Thumb, 12 bytes, Stack size 0 bytes, main.o(i.Delay))
  [Called By]

  - >> main

  GPIO_ConfigPinRemap (Thumb, 70 bytes, Stack size 20 bytes, n32h47x_48x_gpio.o(i.GPIO_ConfigPinRemap))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_ConfigPinRemap
  [Called By]
  - >> main

  GPIO_InitPeripheral (Thumb, 160 bytes, Stack size 20 bytes, n32h47x_48x_gpio.o(i.GPIO_InitPeripheral))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_InitPeripheral
  [Called By]
  - >> LED_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, n32h47x_48x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> LED_Off

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, n32h47x_48x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> LED_On

  GPIO_TogglePin (Thumb, 8 bytes, Stack size 0 bytes, n32h47x_48x_gpio.o(i.GPIO_TogglePin))
  [Called By]

  - >> LED_Blink

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  LED_Blink (Thumb, 16 bytes, Stack size 16 bytes, main.o(i.LED_Blink))
  [Stack]

  - Max Depth = 16
  - Call Chain = LED_Blink
  [Calls]
  - >> GPIO_TogglePin
  [Called By]
  - >> main

  LED_Init (Thumb, 50 bytes, Stack size 40 bytes, main.o(i.LED_Init))
  [Stack]

  - Max Depth = 60
  - Call Chain = LED_Init ⇒ GPIO_InitPeripheral
  [Calls]
  - >> GPIO_InitPeripheral
  - >> RCC_EnableAHB1PeriphClk
  [Called By]
  - >> main

  LED_Off (Thumb, 16 bytes, Stack size 16 bytes, main.o(i.LED_Off))
  [Stack]

  - Max Depth = 16
  - Call Chain = LED_Off
  [Calls]
  - >> GPIO_ResetBits
  [Called By]
  - >> main

  LED_On (Thumb, 16 bytes, Stack size 16 bytes, main.o(i.LED_On))
  [Stack]

  - Max Depth = 16
  - Call Chain = LED_On
  [Calls]
  - >> GPIO_SetBits
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  RCC_EnableAHB1PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32h47x_48x_rcc.o(i.RCC_EnableAHB1PeriphClk))
  [Called By]

  - >> LED_Init

  RCC_EnableAPB2PeriphClk (Thumb, 26 bytes, Stack size 0 bytes, n32h47x_48x_rcc.o(i.RCC_EnableAPB2PeriphClk))
  [Called By]

  - >> main

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  SystemInit (Thumb, 120 bytes, Stack size 8 bytes, system_n32h47x_48x.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetStartupVolt
  [Calls]
  - >> SetSysClock
  - >> SetStartupVolt
  [Address Reference Count : 1]
  - startup_n32h487.o(.text)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32h47x_48x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_n32h487.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 208 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 60
  - Call Chain = main ⇒ LED_Init ⇒ GPIO_InitPeripheral
  [Calls]
  - >> GPIO_ConfigPinRemap
  - >> LED_On
  - >> LED_Off
  - >> LED_Init
  - >> LED_Blink
  - >> Delay
  - >> RCC_EnableAPB2PeriphClk
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetStartupVolt (Thumb, 138 bytes, Stack size 12 bytes, system_n32h47x_48x.o(i.SetStartupVolt))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetStartupVolt
  [Called By]
  - >> SystemInit

  SetSysClock (Thumb, 162 bytes, Stack size 0 bytes, system_n32h47x_48x.o(i.SetSysClock))
  [Called By]

  - >> SystemInit

  ### Undefined Global Symbols