V1.2.0版本
1.修改GPIO初始化函数，删除EXTI相关配置


V1.1.1版本
1. n32g05x_adc.c文件中，ADC_GetFlagStatus()与ADC_GetIntStatus()函数中，新增判断EDNC置位后延时8个ADC_CLK的功能
2. 添加IAR工程
3. 优化RCC例程的CSS中断处理
4. 优化DMA驱动的DMA_DeInit()函数
5. PWR模块的LVR\PVD删除1.8V档位
6. demo中缺少结构体初始化的配置，添加结构体初始化函数
7. 部分demo while(1)死循环优化，涉及I2C/RCC/RTC模块
8. TIM ComplementarySignals demo优化
9. UART GPIO初始化添加IO上拉，中断处理中添加错误标志清除
10. UART_Init函数优化
11. FLASH boot_swap demo优化
12. ADC demo优化ADC初始化配置，ADC_DMA demo优化
13. LED驱动及demo优化


V1.0.0版本
初始版本



/***   For English users   ***/
V1.2.0 version
1. Modify the GPIO initialization function and delete EXTI configurations


V1.1.1 version
1. In the n32G05x_ac.c file, the ADC_CetFlagState() and ADC_CetIntState() functions have added the function of delaying the EDNC setting by 8 ADC_CKs
2. Add IAR project
3. Optimize CSS interrupt handling for RCC routines
4. Optimize the DMA_deInit() function of the DMA driver
5. Remove the 1.8V gear from the LVR/PVD of the PWR module
6. The configuration for structure initialization is missing in the demo. Add a structure initialization function
7. Partial demo while (1) dead loop optimization involving I2C/RCC/RTC modules
8. TIM Complementary Signals demo optimization
9. UART GPIO initialization with IO pull-up added, error flag cleared during interrupt handling
10. UART_Init function optimization
11. FLASH boot_stwap demo optimization
12. ADC demo optimization ADC initialization configuration, ADC-DMA demo optimization
13. LED driver and demo optimization


V1.0.0 version
Initial version