1、功能说明
    通过EXTI来触发时间戳。



2、使用环境

    软件开发环境：KEIL MDK-ARM V5.34.0.0
    硬件开发环境： 
        N32G05x系列：
            基于评估板N32G05xRBQ7_STB V1.0开发
        N32G05x系列：
            基于评估板N32G05xRBL7_STB V1.0开发  



3、使用说明

    系统配置；
        1、时钟源：LSI
        2、EXTI：PB7
        3、串口配置：
                    - 串口为USART1（TX：PA9  RX：PA10）:
                    - 数据位：8
                    - 停止位：1
                    - 奇偶校验：无
                    - 波特率： 115200 


    使用方法：
    1、在KEIL下编译后烧录到评估板，上电后，给PB7灌入高电平，串口打印输出时间戳。
                
                

4、注意事项
    无


1. Function description
    The timestamp is triggered by EXTI.



2. Use environment

	Software development environment: KEIL MDK-ARM V5.34.0.0
    Hardware development environment:
         N32G05x series:
            Developed based on the evaluation board N32G05xRBQ7_STB V1.0
         N32G05x series:
            Developed based on the evaluation board N32G05xRBL7_STB V1.0



3. Instructions for use

    System Configuration;
        1. Clock source: LSI
        2. EXTI: PB7
        3. Serial port configuration:
                    - Serial port is USART1 (TX: PA9 RX: PA10):
                    - Data bits: 8
                    - Stop bit: 1
                    - Parity: none
                    - Baud rate: 115200


    Instructions:
    1. After compiling under KEIL, burn it to the evaluation board. After power-on, pour a high level into PB7, and the serial port will print out the timestamp.
                
                

4. Matters needing attention
    none