1、功能说明

    此例程提供了一种DMA MemtoMem模式用法，用于在FLASH与RAM之间传输数据。  

2、使用环境

    软件开发环境：KEIL MDK-ARM V5.34.0.0
    硬件开发环境： 
        N32G05x系列：
            基于评估板N32G05xRBQ7_STB V1.0开发
        N32G05x系列：
            基于评估板N32G05xRBL7_STB V1.0开发


3、使用说明
	
    1、时钟源：HSE+PLL
    2、主时钟：64MHz
    3、DMA通道：DMA_CH1
    
    4、UART1配置：
            TX  -->  PA9
            波特率：115200
            数据位：8bit
            停止位：1bit
            无校验

    5、测试步骤与现象
        a，编译下载代码复位运行
        b，从串口看打印信息，验证结果

4、注意事项
    无


1. Function description
    This routine provides a DMA MemtoMem mode usage for transferring data between FLASH and RAM.

    
2. Use environment
	Software development environment: KEIL MDK-ARM V5.34.0.0
    Hardware development environment:
         N32G05x series:
            Developed based on the evaluation board N32G05xRBQ7_STB V1.0
         N32G05x series:
            Developed based on the evaluation board N32G05xRBL7_STB V1.0

3. Instructions for use
    1.Clock source: HSE+PLL
    2.Master clock: 64MHz
    3.DMA channel: DMA1_CH1
    
    4.USART1 configuration:
	TX  -->  PA9           
	Baud rate: 115200
	Data bit: 8 bits
	Stop bit: 1bit
	No check

    5.Test steps and phenomena
	A. Compile download code reset run
	B. View the printed information from the serial port and verify the result

4. Precautions
    None
