1、功能说明
    1、通过设定闹钟时间来触发闹钟中断。
    2、通过闹钟标志位来配置IO输出

2、使用环境

    软件开发环境：KEIL MDK-ARM V5.34.0.0
    硬件开发环境： 
        N32G05x系列：
            基于评估板N32G05xRBQ7_STB V1.0开发
        N32G05x系列：
            基于评估板N32G05xRBL7_STB V1.0开发

3、使用说明

    系统配置；
        1、RTC时钟源：LSI
        2、闹钟IO输出：PC13
        3、串口配置：
                    - 串口为UART1（TX：PA9  RX：PA10）:
                    - 数据位：8
                    - 停止位：1
                    - 奇偶校验：无
                    - 波特率： 115200 


    使用方法：
        在KEIL下编译后烧录到评估板，上电，串口按照闹钟设定时间进行打印输出，在PC13口会出现翻转电平。

4、注意事项
    无


1. Function description
    1. Trigger the alarm interrupt by setting the alarm time.
    2. Configure the IO output through the alarm flag bit

2. Use environment

    Software development environment: KEIL MDK-ARM V5.34.0.0
    Hardware development environment:
         N32G05x series:
            Developed based on the evaluation board N32G05xRBQ7_STB V1.0
         N32G05x series:
            Developed based on the evaluation board N32G05xRBL7_STB V1.0


3. Instructions for use

    System Configuration;
        1. RTC clock source: LSI
        2. alarm IO output: PC13
        3. Serial port configuration:
                    - Serial port is UART1 (TX: PA9 RX: PA10):
                    - Data bits: 8
                    - Stop bit: 1
                    - Parity: none
                    - Baud rate: 115200


    Instructions:
        After compiling under KEIL, burn it to the evaluation board, power on, and the serial port will print out the time set by the alarm clock, 
        and the flipped level will appear at port PC13.

4. Matters needing attention
    none