1、功能说明
    1、PVD配置电压产生对应的中断。


2、使用环境

    /* 软件开发环境：当前工程使用的软件工具名称及版本号 */
    IDE工具：KEIL MDK-ARM 5.34.0.0
            IAR EWARM 8.50.1
      
    /* 硬件环境：工程对应的开发硬件平台 */
     N32G033系列：
            基于评估板N32G033K8Q7-1_STB V1.0开发
     


3、使用说明

    系统配置；
        1、时钟源：HSI+PLL
        2、时钟频率：64M
        3、打印：PA9-115200

    使用方法：
        在KEIL下编译后烧录到评估板，把电压调低到PVD设置电压以下，会进入中断，打印"Enter PVD interrupt"。


4、注意事项
    无


1. Function description
    1. The PVD configuration voltage generates a corresponding interrupt.


2. Development environment

    /* Software development environment: the name and version number of the software tool used in the current project */
    IDE tool: KEIL MDK-ARM 5.34.0.0
            IAR EWARM 8.50.1
      
    /* Hardware environment: the development hardware platform corresponding to the project */
     N32G033 series:
            Developed based on the evaluation board N32G033K8Q7-1_STB V1.0


3. How to use

    System Configuration;
        1. Clock source: HSI+PLL
        2. Clock frequency: 64M
        3. Log: PA9-115200

    Instructions:
        After compiling under KEIL, burn it to the evaluation board, lower the voltage to below the LVR setting voltage,
       It will enter the interrupt and print "Enter PVD interrupt".


4. Attention
    none

