Nations.N32G003_Library.1.2.0：
1. 修改EXTI demo中断函数标志位改为获取flag标志
2. 修改SPI FLASH demo中，写字节发送数据后，读数据增加前，增加TE/BUSY标志位查询
3. 优化UART溢出中断问题
4. 优化I2C通信，添加自恢复功能
5. 修改I2C demo中i2c_master_recv函数接收2个字节后清除ACKPOS位
6. 修改SDK中HCLK名称为SYSCLK
7. 删除SDK DBG_STOP函数调用
8. 在TimeBasic6_wakeup demo中，更新中断处理函数，判断EXTI_GetStatusFlag(EXTI_LINE9) != RESET标志位。

Nations.N32G003_Library.1.1.0：
1. 修改Flash_One_Page_Erase函数增加地址判断
2. 修改ADC demo中用ENDCA代替ENDC使用，并增加8个ADC_CLK延时；
3. 修改IWDG demo，使用BSP里面的log.c文件
4. 优化UART驱动的波特率计算方式
5. 优化各模块例程中的while循环及错误处理
6. 更新RCC驱动的时钟获取函数

Nations.N32G003_Library.1.0.1：
1. FLASH USER3 添加LVRRSTEN功能
2. GPIO添加GPIO_AF8_UART2: PA9复用为UART2_RX
3. SPI例程修改BaudRatePres和GPIO引脚
4. 添加IAR例程
5. UART例程修改RX GPIO模式 

Nations.N32G003_Library.1.0.0：
初始版本
-------------------------------------------------------
Nations.N32G003_Library.1.2.0：
1. Modify the EXTI demo to change the interrupt function flag to obtain the flag status.
2. Modify the SPI FLASH demo to add TE/BUSY flag query before reading data after sending data in the write byte operation.
3. Optimize the UART overflow interrupt issue.
4. Optimize I2C communication and add a self-recovery function.
5. Modify the i2c_master_recv function in the I2C demo to clear the ACKPOS bit after receiving two bytes.
6. Rename HCLK to SYSCLK in the SDK.
7. Remove the DBG_STOP function call from the SDK.
8. In the TimeBasic6_wakeup demo, update the interrupt handler to check the EXTI_GetStatusFlag(EXTI_LINE9) != RESET flag.

Nations.N32G003_Library.1.1.0：
1. Modify Flash_One_Page_Erase funtion to add address judgment
2. Modify ADC demo, use ENDCA flag replace ENDC flag, and add 8 ADC_CLK delay；
3. Modify IWDG demo，USB log.c file in BSP
4. Optimize the baud rate calculation of the UART driver
5. Optimize the while loop and error handling in each module routine.
6. Update the clock acquisition function of RCC driver.

Nations.N32G003_Library.1.0.1：
1. FLASH USER3 LVRRSTEN funtions modify
2. GPIO add GPIO_AF8_UART2: PA9 as UART2_RX
3. SPI demo modified BaudRatePres and GPIO pins
4. Adds IAR demo
5. UART demo modified RX GPIO mode 

Nations.N32G003_Library.1.0.0：
Initial release
