1. 功能说明
    此例程展示在 RT_Thread 系统创建 ADC 设备

2. 使用环境
    硬件环境：工程对应的开发硬件平台 
    开发板：   N32WB45xL_EVB_V1.1

3. 使用说明
    描述相关模块配置方法；例如:时钟，I/O等 
         1. SystemClock：144MHz
         2. GPIO：LED:D1--PD0
                        ADC:
                               PA0选择为模拟功能ADC1转换通道
                               PA2选择为模拟功能ADC1转换通道
                        日志：TX--PA9  RX--PA10，波特率：115200

    描述Demo的测试步骤和现象 
         1. 编译后下载程序复位运行
         2. 本例程在main()里面创建两个线程，test0 线程和 test1 线程，test0 线程用于控制 D1 500ms闪烁，在test1线程中测试ADC设备,测量PA0和PA2引脚电压，通过串口打印结果

4. 注意事项
    无

1. Function description
    This routine shows how to create an ADC device on the RT_Thread system

2. Use environment
    Hardware environment: development hardware platform corresponding to the project 
    Development board:      N32WB45xL_EVB_V1.1

3. Instructions for use
    Describe the configuration method of related modules; for example: clock, I/O, etc. 
        1. SystemClock: 144MHz
        2. GPIO: LED:D1--PD0
                     ADC:
                            PA0 is selected as the analog function ADC1 conversion channel
                            PA2 is selected as the analog function ADC1 conversion channel
                     Log: TX--PA9 RX--PA10 Baud rate: 115200

    Describe the test steps and phenomena of Demo 
        1. After compiling, download the program to reset and run;
        2. This routine creates two threads in main(), test0 thread and test1 thread, test0 thread is used to control D1 500ms flashing, 
            test the ADC device in test1 thread, measure the pin voltage of PA0 and PA2, and print the result through serial port

4. Matters needing attention
    None.