1、功能说明

    此例程展示了通过I2C模块与外部EEPROM的通信。   

2、使用环境

   软件开发环境：
    IDE工具：KEIL MDK-ARM 5.34.0.0
             IAR EWARM 8.50.1
    
    硬件环境：
     N32G033系列：
            基于评估板N32G033K8Q7-1_STB V1.0开发


3、使用说明
	
    1、主时钟：64MHz
    2、I2C1 配置：
            SCL   -->  PB6          
            SDA   -->  PB7         
            CLOCK:400KHz
            
    3、USART1配置：
            TX  -->  PA9   
            RX  -->  PA10           
            波特率：115200
    
    4、测试使用EEPROM型号:
	    AT24C04（容量4kb）
        

    5、测试步骤与现象
        a，检查EEPROM连接
        b，编译下载代码复位运行
        c，从串口看打印信息，验证结果

4、注意事项
   1. MCU 作为主机发送且为 7 位地址模式时，从机地址不能配置成 0xF0、0xF2、0xF4 或 0xF6。

1. Function description

     This example demonstrates the communication with the external EEPROM through the I2C module.

2. Development environment

    Software development environment:
    IDE tool: KEIL MDK-ARM 5.34.0.0
            IAR EWARM 8.50.1
    
     Hardware environment:
     N32G033 series:
            Developed based on the evaluation board N32G033K8Q7-1_STB V1.0


3. How to use

     1. Main clock: 64MHz
     2. I2C1 configuration:
             SCL --> PB6
             SDA --> PB7
             CLOCK: 400KHz
            
     3. USART1 configuration:
             TX --> PA9
             RX --> PA10
             Baud rate: 115200
    
     4. Test using EEPROM model:
            AT24C04 (capacity 4kb)
        

     5. Test steps and phenomena
         a, check the EEPROM connection
         b, compile and download the code, reset and run
         c, view the print information from the serial port and verify the result

4. Attention
    1. When the MCU is sent as a host and in 7-bit address mode, the slave address cannot be configured as 0xF0, 0xF2, 0xF4, or 0xF6.